Try getting signal with a different probe on my setup, If I can get signal then I now the probe must be messed up. Try completely rebuilding the probe with a new box that’s more sound with screws and everything.

When moving the RA10 (4.81MHz) from Mikes setup to the Rack Mounted NMR machine, no signal is received. Yet at Mikes setup it works fine, with same parameters and attenuation.

Working values:

For CPMG : 23DB, and 17DB with 3.6us

9090: 17DB 17DB, with 1.8us